input:

qcc3007.xuv

this file is available after you use adk3.5 downloading and running the source code program.

run: 4.gnerate\_bin\_for\_upgarde.bat

get: CubicSpeaker\_3007\_upg\_signed.bin

to be over written to

CSPKDS16WriteBT0.2.bin

CSPKDS24WriteBT0.2.bin

CSPKDS10WriteBT0.2.bin